breadboard collected

- 4 leg push into breadboard

- have to be careful when connecting

- play around with it and see what happens

three parameters:

- value

- timestamps (epach converter)

- context

1 dot = value, timestamp, context

Use HTTP for programming

HTTP:

- Host

- Path

- Headers

- Payload

understand the http