**Ubidots Communications**

1. Connect to Ubidots Cloud (URL?)
   1. *Python code format?*
2. Do a handshake to start a communication session
   1. Create a Token based on our Ubidots Account (Ubidots ID?)
      1. *Python code format?*
   2. Send a token to start a session in UbiDots Cloud
      1. *Python code format?*
3. Loop while (condition is true)
   1. Send a (gas) data point to our Ubidot Cloud storage
4. Close the session to Ubidots Cloud
5. Destroy the token